**NEW! Chem-Pro® CD1 Multi-Diaphragm Metering Pump**

The Chem-Pro® CD1 offers a top performing solution to the problem of dosing with gas forming chemical, such as peracetic acid or sodium hypochlorite.

The CD1 Dual Diaphragm Hyperlink Drive Technology pumps chemicals continuously, is self-priming, and will not vapor lock. CD1 is engineered for zero maintenance, including the patented ultra-durable diaphragm, called DiaFlex®. This exclusive single layer diaphragm has been designed to last the life of the pump.

Additional benefits include: The energy efficient brushless DC variable speed motor that helps achieve a large turndown ratio for extreme accuracy. CD1 has a feed rate of up to 7.20 GPH (27.26 LPH), leak detection, simple installation and setup, and there are fittings for multiple configuration types.

The Chem-Pro® CD1 provides a high performance solution for precisely dosing harsh chemical.

Submitted by:

Blue-White Industries

5300 Business Drive

Huntington Beach, CA USA 92649

Tel. 714-893-8529

Email: info@blue-white.com

URL: www.blue-white.com