**NEW! Chem-Pro® CD3 Multi-Diaphragm Metering Pump**

The Chem-Pro® CD3 offers a top performing solution to the problem of dosing with gas forming chemical, such as peracetic acid or sodium hypochlorite.

The CD3 Dual Diaphragm Hyperlink Drive Technology pumps chemicals continuously, is self-priming, and will not vapor lock. CD3 is engineered for zero maintenance, including the patented ultra-durable diaphragm, called DiaFlex®. This exclusive single layer diaphragm has been designed to last the life of the pump.

Additional benefits include: The energy efficient brushless DC variable speed motor that helps achieve a large turndown ratio for extreme accuracy. CD3 has a flow range of .05 to 53 GPH (0.2 to 200 LPH), leak detection, simple installation and setup, and there are fittings for multiple configurations.

The Chem-Pro® CD3 is provides an high performance solution for precisely dosing harsh chemical.

Submitted by:

Blue-White Industries

5300 Business Drive

Huntington Beach, CA USA 92649

Tel. 714-893-8529

Email: info@blue-white.com

URL: www.blue-white.com