**New High Volume, Energy Efficient Chemical Feed Pump**

The New FLEXFLO® A5 Peristaltic Metering Pump has the capability to deliver chemical feed up to 9 gallons per minute at only 75 RPM motor speed. This not only serves to greatly increase tube life, it is also incredibly energy efficient.

FLEXFLO A5 is a fully enclosed and easily configurable pump that does not require external control devices to operate. It features a large 5″ display for easy viewing with simple and intuitive touchscreen controls and icon-driven menu navigation. A5 remote control signal options include Pulse, 4-20mA, Modbus TCP, EtherNet/IP™, and PROFIBUS for enhanced supervision and automation for critical metering and transfer applications.

The A5’s patent pending roller assembly reduces pulsations by 80% and pump tube assemblies are dual channel and deliver excellent tube life.

WEFTEC Booth 1817

https://www.blue-white.com/product/a5-peristaltic-metering-pump/